33um plastic absorber; 100% CO2; 10 000 events

33um plastic absorber; 50% CO2; 10 000 events no plastic absorber; 0% CO2; 10 000 events