Definition of U and V planes in MOFIA geometry files

Author: K.Olchanski Date: 26 Nov 2001 The planes are labeled according to the coordinate they measure: "X-planes" measure X, "Y-planes" measure Y, "U-planes" measure U and "V-planes" measure V. In the MOFIA geometry file, the U and V planes are made out of X-planes by rotating them around the Z-axis, as shown in this figure (note the location of wire 1):

Figure 1. Planes rotated by +/-45 and +/-135 degrees

Table 1. Rotation angles used in TWIST geometry files

Angle Plane type +45 upstream PC and DC U planes -45 upstream PC and DC V planes -135 downstream PC, DC and target PC U planes +135 downstream PC, DC and target PC V planes

1

2